April 29, 2020

«Contact\_Name»

«User\_Name»

«User\_Address»

Re: Surcharge Limits Calculations

«Contact\_Title»,

This letter is to inform you of the surcharge calculations with respect to «User\_Name» («USER\_CODE») for the «Month\_Year» monitoring period. The purpose of the surcharge program is to accurately and equitably allocate costs to those who generate high strength wastewater. Regardless of monthly average permit limits, surcharge fees are assessed when monthly average results are above City Code surcharge thresholds. The following tables summarizes surcharge calculation values and «SIU\_CODE»’s monthly average results used to determine the surcharge calculation.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Surcharge Formula Thresholds and Rates | | | | | |
| Pollutant | TSS | CBOD | NH3-N | T-Phos | O&G |
| Threshold | 200 | 200 | 15.0 | 4.0 | 100 |
| $ / lb | 0.14 | 0.13 | 0.70 | 5.08 | 0.14 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Surcharge Calculation based on a total monthly flow of «Flow» million gallons | | | | | |
| Pollutant | TSS | CBOD | NH3-N | T-Phos | O&G |
| Monthly Average mg/L | «TSSppm» | «CBODppm» | «NH3Nppm» | «TPhosppm» | «O&Gppm» |
| Surcharge $ | «TSS\_Charge» | «CBOD\_Charge» | «NH3N\_Charge» | «TPhos\_Charge» | «O&G\_Charge» |

Surcharge $ = Flow x 8.34 x ((0.14 x (TSS - 200)) + (0.13 x (CBOD-200)) + (0.70 x (NH3-N–15.0)) +

(5.08 x (T-Phos – 4.0)) +(0.14x(O&G–100)))

The total surcharge amount of **$«Total\_Surcharge»** will be added to «USER\_CODE»’s next water bill. Please note that surcharges **are not** permit violations. Any permit violations for the monitoring period are dealt with separately. If you have any questions regarding this surcharge letter, please contact me.

Sincerely,

Ben Franklin, Coordinator

Copy: G. Washington, J. Adams, T. Jefferson, A. Lincoln, Filed F:\Surcharges

E. Warren, H. Hoover«Contact2»«Contact3»